{"text_format":"1","workbook":"xlsx","n_sheets":16,"sheets":["Home","AR Server - Cloud Portal & DB ","AR System Mid Tier","AtriumCoreWebRegistryComponents","BSA-AppServer&Console","BSA-FileServer","BSA-MultipleAppServer","AO-CDP","AO-CDP (HA)","BNA","Cloud Database Extensions","Cloud Platform Manager","Cloud Portal AR Extensions","PXE Server","BSA-AdvRep","BNA-Device Agent"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Home","index":0,"n_rows":19,"n_cols":1,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
["Instructions for Using the Planning Spreadsheets"]
[]
["The tabs in this file contain lists of fields that you will encounter with each installer.  Each tab corresponds to a particular installer. Save this file, and complete the worksheet before starting each installer."]
[]
["BMC AR System Server - Cloud Portal and Database (SQL Server)"]
["BMC Remedy Mid Tier"]
["BMC Atrium Core Web Registry Components"]
["BMC Server Automation - App Server & Console"]
["BMC Server Automation - File Server"]
["BMC Server Automation - Multiple App Server"]
["Atrium Orchestrator - Configuration Distribution Peer"]
["Atrium Orchestrator - Configuration Distribution Peer (HA)"]
["Cloud Database Extensions"]
["BMC Network Automation"]
["Cloud Platform Manager"]
["Cloud Portal AR Extensions"]
["PXE Server"]
["BMC Server Automation - Advanced Repeater"]
["BMC Network Automation - Device Agent"]

{"sheet":"AR Server - Cloud Portal & DB ","index":1,"n_rows":63,"n_cols":3,"rows_kept":63,"cut":false,"hidden":false,"merged":[[0,0,0,2]]}
["The BMC AR System Server - Cloud Portal & Database installation consists of the following components:\n1. BMC Remedy ITSM Suite Preconfigured Stack 8.1.01\n2. AR Post Install Config"]
[]
["Field in Install Planner","Default value displayed ","Comments"]
["Remote Directory Selection","C:\\Program Files\\BMC Software","Installer checks if you have adequate disk space  to install BMC Remedy ITSM Suite Preconfigured Stack 8.1.01."]
["AR System Java Platform Information"]
["64-bit Oracle JRE Path","Detected and set by installer","Install JRE 1.7"]
["AR System Server Database Information",null,"Selected by default and cannot be disabled."]
["Unicode Character Strings",null,"Cannot modify this value. "]
["Authentication","SQL Server Authentication selected by default. If you choose Windows authentication, enter your Windows login ID and password."]
["Host name or IP address (of database server)",null,"The computer from which you are installing must be able to ping  the name or address you provide. (Server host name does not need to be a fully qualified host name.)"]
["AR System Server DB port",1433]
["AR System Server DB Instance Name","Enter required value","Your DBA may have created and named this instance."]
["AR System Server DB Name","ARSystem","Cannot modify this value. "]
["AR System Server DB Log-in ID","ARAdmin"]
["AR System Server DB Password","Entered by default(AR#Admin#)","Password can be changed."]
["AR System Server Administrator Information"]
["AR System Server Administrator Name","Demo","Cannot modify this value. "]
["AR System Server Server Password","none"]
["AR System Server Server TCP Port","Optional value","Displays the BMC Remedy AR System Server TCP Port Number you entered in the BMC Remedy AR System Portmapper and TCP Port Information panel."]
["AR System Server server name alias ","Entered by default","Must be registered in the DNS server."]
["Host Name or IP address (of physical system)","Entered by default","With fully-qualified domain name"]
["DBMS Administrator Information"]
["SQL Server Administrator Login","Enter required value","The specified database user must have the DBA privileges."]
["SQL Server Administrator Password","Enter required value","Specify the database administrator password."]
["AR System Server Database File Information"]
["AR System Server DB Name","ARSystem","Cannot modify this value"]
["Datafile Name","ARSys","You can modify the default datafile name displayed in this field if required."]
["Logfile Name","ARSysLog","You can modify the default datafile name displayed in this field if required."]
["Language Selection"]
["English","Entered by default","English only selected by default to speed up installation. "]
["All Languages","Optional value","Choose now if you need to install additional languages. If you add languages later, you must run each of the standalone product installers in the ITSM Suite. "]
["AR System Password Information"]
["Local DSO User Password","Enter required value","The DSO password must not be greater than 8 characters. You can change these values later in BMC Remedy Administrator Console. "]
["Application Server Password","Enter required value","You can change these values later in BMC Remedy Administrator Console. "]
["Mid-Tier Administration Password","Enter required value","You can change these values later in BMC Remedy Administrator Console. "]
["Plugin Port Information"]
["NE Plugin Port",9555,"Port number used by the Normalization Engine plugin."]
["Atrium Plugin Port",9556,"Port number used by the Atrium plugin."]
["AR System Server RMI Port and RPC Program Number"]
["Flashboards Server RMI Port",1099,"You can keep the default values. For more details, check the BMC Remedy AR System documentation."]
["Flashboards Server RPC Program Number",0,"You can keep the default values. For more details, check the BMC Remedy AR System documentation."]
["Email Engine RMI Port",1100,"You can keep the default values. For more details, check the BMC Remedy AR System documentation."]
["Email Engine RPC Program Number",0,"You can keep the default values. For more details, check the BMC Remedy AR System documentation."]
["Tomcat Information"]
["Select Yes or No","Yes","You can select No if Tomcat is already installed. Note: If you select No, you will have to provide the existing location of the Tomcat installation."]
["Tomcat Installation Directory"]
["Tomcat Installation Directory","C:\\Program Files\\Apache Software Foundation\\Tomcat6.0","You can modify the default path displayed in this field if required."]
["Tomcat Configuration"]
["Initial Memory Pool","1536 MB"]
["Maximum Memory Pool","2048 MB"]
["HTTP Port",8080]
["BMC Remedy Developer Studio - Workspace Folder Selection"]
["Select a destination for your workspace folder","C:\\Users\\Administrator\\Developer Studio"]
["AR System Server License Information"]
["AR Server License Key","Enter required value"]
["License Expiration Date","Optional value","Required only if you are using a temporary license."]
["License Qualifier","Optional value","This field is used to further identify license behavior. Do not modify the contents of this field unless instructed to do so by BMC or a qualified BMC partner."]
["AR Post Install Configuration component details"]
["BMC Remedy AR System User inputs"]
["AR System Server Administrator Name",{"$f":"$B$17","v":"Demo"},"Entered by default. If not, then specify the adminstrator name which you specified earlier while installing the BMC AR System Server - Cloud Portal and Database."]
["AR System Server Password",{"$f":"$B$18","v":"none"},"Entered by default. If not, then specify the adminstrator name which you specified earlier while installing the BMC AR System Server - Cloud Portal and Database."]
["AR System Server TCP Port",0,"Entered by default"]
["AR System Server Name Alias","Entered by default","Entered by default"]

{"sheet":"AR System Mid Tier","index":2,"n_rows":22,"n_cols":3,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["Field in Install Planner","Default value displayed","Comments"]
["Remote Directory Selection","C:\\Program Files\\BMC Software\\ARSystem ","Select the location on your computer where you want to install the BMC Remedy AR System Mid Tier."]
["Java Platform Information"]
["64-bit 1.7 Oracle JRE path","Entered by default","Specify the location where you installed Oracle JRE."]
["AR System Server List"]
["AR Server","Enter required value","Add the AR Server(s) for which you want to install a Mid Tier web server, for example, the BMC AR System Server - Cloud Platform and Database host. Click Add to add the information, or select an AR System server and click Remove to remove it."]
["TCP",0,"The field is optional."]
["RCP",null,"The field is optional."]
["Mid Tier Pwd","Enter required value","Provide the mid tier administrator Password that you provided during the BMC AR System & IT Service Management Suite - Primary installation."]
["Pre-Load","Selected by default","For best system performance, although caching might slow the mid tier response temporarily at first. "]
["Tomcat Information"]
["Select Yes or No","Yes, selected by default","Select Yes or No depending on your requirement."]
["Tomcat Installation Directory"]
["Tomcat Installation Directory","C:\\Program Files\\Apache Software Foundation\\Tomcat6.0"]
["Tomcat Configuration parameters"]
["Initial Memory Pool (MB)",2048,"You can change the value if required."]
["Maximum Memory Pool (MB)",2048,"You can change the value if required."]
["HTTP Port",8080,"You can change the value if required."]
["Preference, Home Page, and DVM Server Information"]
["Preference Server","Enter required value","The name of the AR System server designated as a preference server. You can specify more than one server if you need multiple preference servers to support different departments or business units. If you enter more than one preference server, the system searches the list until it finds the first preference server that matches the user name and uses that server as the preference server. A fully qualified server name is not valid in this field.\nNote: All servers designed as preference servers must be included in the AR System Server list on the AR Server Settings page."]
["Home Page","Enter required value","The server that contains the home page that you want to open in the browser when the user logs in. The home page URL is: http://midTierServer/contextPath/home\nThe home page server must already in the list of AR System servers on the AR Server Settings page.  The mid tier searches this server for the designated or default home page. This server is used globally if you have not selected a home page server in the AR System User Preference form. A home page server specified in the AR System User Preferences form takes precedence over the server set here."]
["Data Visualization","Enter required value","The name of the AR System server designated as a data visualization module server. You can specify more than one server if you need to copy the modules to another server as a backup in case the first module server goes down. To add or update module servers, enter the name of each server that you want to designate as a module server. A fully qualified server name is not valid in this field.\nNote: All servers designed as module servers must be included in the R System Server list on the AR Server Settings page."]

{"sheet":"AtriumCoreWebRegistryComponents","index":3,"n_rows":19,"n_cols":3,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
["Field in Install Planner","Default value displayed","Comments"]
["Remote Directory Selection"," C:\\Program Files\\BMC Software\\Atrium Web Registry ","Select the location on your computer where you want to install the Atrium Core Web Registry components."]
["AR System Server Information",null,"AR System server created with BMC AR System Server - Cloud Portal and Database"]
["User Name","Demo","This user must have AR System administrator privileges on the AR System server created with BMC AR System Server & IT Service Mgt. Suite . The version of the AR System server must be 7.6.04 or higher. "]
["Password","none"]
["Port Number",0]
["AR Server Host Name","Entered by default.","BMC AR System Server - Cloud Portal and Database host"]
["Tomcat Installation Confirmation"]
["Select Yes or No","Yes, selected by default","You cannot use the Tomcat servlet installed with the Mid Tier or the ITSM Stack."]
["Tomcat Information"]
["Tomcat Installation Directory","C:\\Program Files\\Apache Software Foundation\\Tomcat6.0"]
["Tomcat Information"]
["HTTP Port",8080]
["HTTPS Port",7776]
["JDK/JRE Path","For example, C:\\Program Files\\Java\\jre7","Specify the location where you installed Java JRE."]
["UDDI registry information"]
["User name","admin","You can change this value if required."]
["Password","none","Value is encrypted. For example, admin."]
["Retype User Password","none","Value is encrypted. For example, admin."]

{"sheet":"BSA-AppServer&Console","index":4,"n_rows":47,"n_cols":3,"rows_kept":47,"cut":false,"hidden":false,"merged":[[0,0,0,2]]}
["BMC Server Automation - App Server & Console installation consists of the following components:\n1. BMC Server Automation Application Server\n2. BMC Server Automation Console\n3. BMC Server Automation Post Install Configuration"]
[]
["BMC BladeLogic Operations Manager component details"]
["Field in Install Planner","Default value displayed ","Comments"]
["Remote Directory Selection"]
["Remote Destination Directory","C:\\Program Files\\BMC Software\\BladeLogic"]
["Database Information"]
["Host Name or IP Address","Entered by default","Specify the database user that you want to created for BMC Server Automation."]
["Database Port",1433]
["DBA User","sa","Ask your DBA for information about the database user."]
["DBA Password","Enter required value","Ask your DBA for information about the database password."]
["Confirm DBA Password","Enter the password again"]
["Database User and Datafile Configuration",null,"Enter the following credentials  to create the BMC BladeLogic Operations Manager database and database user. If you did not pre-create a database and user, the installer creates them using the credentials that you specify here."]
["BladeLogic User","bladelogic"]
["User Password","Enter required value"]
["Confirm User Password","Enter required value"]
["Database Name","BLADE"]
["Database Character Set","NCHAR selected by default","You can select CHAR if required. Note: There are 2 sets of database files for BMC Server Automation -- Application Server & Console, one for each character set.  The selection determines which file is used when installing the schema."]
["Database Datafile","C:\\Program Files\\Microsoft SQL Server\\MSSQL10_50.MSSQLSERVER\\MSSQL\\DATA\\bladelogic.mdf","Make sure these values match your environment. "]
["Initial Database Datafile Size (GB)",5,"You can change the Datafile size if required."]
["Database Logfile","C:\\Program Files\\Microsoft SQL Server\\MSSQL10_50.MSSQLSERVER\\MSSQL\\DATA\\bladelogic_log.ldf","Make sure these values match your environment. "]
["Initial Database Logfile Size (GB)",2,"You can change the Logfile size if required."]
["Certificate Password information"]
["Password","Enter required value","Create a password for the self-signed certificate for the Application Server to use the Secure Socket Layer (SSL)."]
["Verify","Enter the password again"]
["File Server Information"]
["File Server Name","Entered by default","Specify the name of the BSA host. "]
["File Server Storage Location","C:\\Program Files\\BMC Software\\BladeLogic\\storage"]
["Application Server JVM Settings"]
["Max (MB) ","2048 (by default)","Specify the maximum JVM heap size for the Application Server. Valid values range from 512 MB to 4096 MB."]
["Notification Servers Information",null,"This fields are optional"]
["SMTP Server","SMTP Server name","You can configure an SMTP relay through which notification emails will be sent from the Configuration Manager. You can also configure the address from which notification emails originate. If you do not plan to use email notifications, you can skip this step."]
["Email From","Email From","Specify the email from which the notification should originate."]
["SNMP Server","SNMP Server name","You can configure an SNMP destination to which all SNMP traps will be sent. If you do not plan to use SNMP trap notifications, you can skip this step."]
["SNMP Port",161]
["BMC Server Automation Post Install Configuration"]
["BMC AR System Server - Cloud Portal and Database Connection Settings"]
["AR System Server Name","Enter required value","Specify the BMC AR System Server - Cloud Portal and Database host name."]
["AR System Server User Account Name","Demo"]
["AR System Server Server Password ","Enter required value"]
["Confirm AR System Server Server Password ","Enter the password again"]
["AR System Server Server Port   ",0]
["User Passwords Information"]
["Password","Enter required value","The RBACAdmin user is the super-user who has full permission in managing Configuration Manager users. You must set the password so that this user is protected."]
["Confirm Password","Enter the password again"]
["Password","Enter required value","The BLAdmin user is the super-user that has Read access on every Configuration Manager object. You must set the password so that this user is protected."]
["Confirm Password","Enter the password again"]

{"sheet":"BSA-FileServer","index":5,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["Field in Install Planner","Default value displayed","Comments"]
["File Server Location","C:\\Program Files\\BMC Software\\Bladelogic\\storage"]

{"sheet":"BSA-MultipleAppServer","index":6,"n_rows":23,"n_cols":3,"rows_kept":23,"cut":false,"hidden":false,"merged":[]}
["Field in Install Planner","Default value displayed","Comments"]
[]
["Remote Directory Selection","C:\\Program Files\\BMC Software\\BladeLogic","For installing BMC BladeLogic Operations Manager"]
["Database Information"]
["Host Name or IP Address","Entered by default","Specify the database user that you want to created for BMC Server Automation."]
["Database Port",1433]
["Database Name ","Entered by default","If you launched the installer from the same host on which you launched the BMC Server Automation -- Application Server & console installation , the dataase values are auto-populated."]
["Database User Name","Entered by default","Ask your DBA for information about the user."]
["Database User Password","Enter required value","Ask your DBA for information about the password."]
["Confirm User Password","Enter the password again"]
["Certificate Password Information",null,"Create a password for the self-signed certificate for the Application Server to use the Secure Socket Layer (SSL). This password must match the keystore password that you specified during the Primary BMC Server Automation--Application Server & Console installation."]
["Password","Enter required information","Password entered by default"]
["Verify","Enter required information"]
["File Server Information"]
["File Server Name","Entered by default","Specify the name of the host where you installed the BMC Server Automation - File Server. "]
["File Server Storage Location","C:\\Program Files\\BMC Software\\BladeLogic\\storage"]
["Application Server JVM Settings"]
["Max (MB) ",1024,"Specify the maximum JVM heap size for the Application Server. Valid values range from 512 MB to 4096 MB."]
["Notification Servers Information",null,"This fields are optional"]
["SMTP Server","SMTP Server name","Optionalally, configure the SMTP relay through which notification emails will be sent to the Configuration Manager. If you do not plan to use email notifications, you can skip this input."]
["Email From","Email From"]
["SNMP Server","SNMP Server name","Optionally, you might configure an SNMP destination to which all SNMP traps will be sent. If you do not plan to use SNMP trap notifications, you can skip this input."]
["SNMP Port",161]

{"sheet":"AO-CDP","index":7,"n_rows":68,"n_cols":3,"rows_kept":68,"cut":false,"hidden":false,"merged":[[0,0,0,2]]}
["The BMC Atrium Orchestrator - Configuration Distribution Peer (CDP) installation included the following components:\n1. BMC Atrium Orchestrator Access Manager and Repository\n2. BMC Atrium Orchestrator CDP\n3. BMC Cloud Lifecycle Content\n4. BMC Server Automation Console\n5. Atrium Orchestrator Post Install Configuration"]
[]
["BMC Atrium Orchestrator Access Manager & Repository component details"]
["Field in Install Planner","Default value displayed","Comments"]
["Remote Destination Directory "]
["Remote Directory Selection","C:\\Program Files\\BMC Software\\AO-Platform\\AMREPO","Select the location on your computer where you want to install BMC Atrium Orchestrator Access Manager and Repository."]
["Access Manager Web Server Settings"]
["HTTP Port",9090,"web server port"]
["Shutdown Port",9005]
["Access Manager Communication Settings"]
["Web Server Protocol","http","You can also choose https"]
["Host Name or IP Address","Entered by default","Can be FQDN"]
["Web Server Port Number",9090,"same as HTTP Port"]
["Communications Port Number",61616]
["BMC Atrium Orchestrator - CDP information"]
["Remote Destination Directory ","C:\\Program Files\\BMC Software\\AO-Platform\\CDP"]
["Configuration Distribution Peer (CDP) Web Server Settings"]
["HTTP Port",28080]
["Shutdown Port",28005]
["Configuration Distribution Peer Settings"]
["Environment Name","ENV1"]
["Administrator Password","admin123","The password is encrypted. You cannot modify the password in the installer."]
["Grid Name","GRID1"]
["Grid Type","Development","You can also select QA Test, Pre production, or Production"]
["Grid Log Level","DEBUG","You can also select ERROR, INFO, OFF, or WARN"]
["CDP Name","CDP1"]
["Certficate Holder Name","BMC Software"]
["Certificate Holder Password","Enter required values","Assign a password longer than 6 characters"]
["Peer Comunications Port Number",28081]
["Repository Communications Settings"]
["Web Server Protocol","http","You can also choose https"]
["Host Name or IP Address","Entered by default","Host name of Atrium Orchestrator -- Configuration Distribution Peer."]
["Web Server Port Number",9090]
["BMC Cloud Lifecycle Management Content"]
["Remote Destination Directory ","C:\\Program Files\\BMC Software\\AO-Content"]
["Repository Communications Settings"]
["Web Server Protocol","http","You can also choose https"]
["Host Name or IP Address","Entered by default","Host name of Atrium Orchestrator -- Configuration Distribution Peer."]
["Web Server Port Number",9090]
["Repository User","admin"]
["Repository Password","admin123","Password is encrypted."]
["BladeLogic Server Automation Console"]
["Remote Destination Directory ","C:\\Program Files\\BMC Software\\BladeLogic"]
["Atrium Orchestrator Post install config"]
["ARS Adapter Information Panel",null,"The ARS adapter is enabled using the orchestration user that is created during the BMC AR System Server and Cloud Portal and Database installation."]
["Enable ARS Adapter","Select this option","Cleared by default"]
["AR Enterprise Host Name","Entered by default","Host of BMC AR System Server & IT Service Mgt. Suite"]
["Orchestration User Name","Entered by default and cannot be edited","orchestrationuser"]
["Orchestration Password","Entered by default and cannot be edited","aouser -- Value is encrypted"]
["AR Enterprise Host Port",0]
["BladeLogic Adapter Information Panel"]
["Enable BladeLogic Adapter","Select this option","Cleared by default"]
["BMC Server Automation - App Server & Console","Entered by default","The name of the host on which you installed BMC Server Automation - Application Server & Console."]
["Port",10840]
["Default User Role","BLAdmins","Entered by default"]
["Profile Name","defaultProfile","Entered by default"]
["SRP User Name","BLAdmin","Entered by default"]
["SRP Password","Enter required value"]
["Netapp Actor Adapter Information Panel"]
["Enable Netapp Actor Adapter","Select this option","Selected by default"]
["DFM Server Hostname/IP","Enter required values"]
["DFM Server Username","Enter required values"]
["DFM Server Password","Enter required values"]
["DFM Protocol","Enter required values","http or https"]
["Port","Enter required values","8088 for http protocol and 8488 for https protocol"]
["High Availability Configuration Distribution Peer (HACDP) Peer Name Information",null,"If you also installed this product during this session."]
["CDP Machine","Entered by default"]
["CDP Peer Name","Enter required values","Enter a name that is not the same as CDP Peer name, for example, PEER2."]

{"sheet":"AO-CDP (HA)","index":8,"n_rows":18,"n_cols":3,"rows_kept":18,"cut":false,"hidden":false,"merged":[[0,0,0,2]]}
["The BMC Atrium Orchestrator - Configuration Distribution Peer (CDP)installation included the following components:\n1. BMC Server Automation Console\n2. BMC Atrium Orchestrator CDP"]
[]
["BMC Server Automation Console component details"]
["Field in Install Planner","Default value displayed ","Comments"]
["Remote Directory Selection"]
["Remote Destination Directory","C:\\Program Files\\BMC Software\\BladeLogic","Select the location on your computer where you want to install BMC BladeLogic Server Automation Console."]
["BMC Atrium Orchestrator Configuration Distribution Peer"]
["Web Server Settings"]
["HTTP Port",58080]
["Shutdown Port",58005]
["Peer to Configuration Distribution Peer Settings",null,"You cannot modify these Peer to Configuration Distribution Peer Settings."]
["Web Server Protocol","http"]
["CDP User Name","Entered by default"]
["CDP Administrator Password","Entered by default","The password by default is admin123.  You cannot modify this value. "]
["Host Name or IP Address","Entered by default"]
["CDP Web Server Port Number",28080]
["Grid Name","GRID1"]
["This Peer's Name","Entered by default"]

{"sheet":"BNA","index":9,"n_rows":80,"n_cols":3,"rows_kept":80,"cut":false,"hidden":false,"merged":[]}
["Field in Install Planner","Default value displayed ","Comments"]
["Data Directory Information"]
["Data Directory","C:\\BCA-Networks-Data"]
["OS User Account Information"]
["Create User Account","Unchecked by default","Check this option if you are not using the Precreate database option in the installer for the BMC Network Automation installation. The installer creates a OS user during the installation."]
["User Name","Enter required information","For example, bna_user. Create this user account before you start BBNA installation. "]
["Password","Enter required information","Create the password for this user account before you start BBNA installation. "]
["Confirm Database Password",null,"Confirm the password you specified in the previous text box."]
["Windows Domain","Required on Windows only","Do not enter an IP address."]
["Web Server Information"]
["HTTPS Port Number",11443]
["Control Port Number",9112]
["Redirect HTTP Requests to HTTPS","Selected by default - HTTP Port Number is 9595","Clear the redirect check box, if you do not want to redirect HTTP requests to HTTPS"]
["HTTP port",9595]
["Database Information"]
["Database Type","Entered by default","Select Microsoft SQL Server or Oracle."]
["Host Name","Entered by default","Host entered by default"]
["Port Number",1433]
["Create New Database","Unchecked by default","Check this option if you are not using the Precreate database option in the installer for the BMC Network Automation installation. The installer creates a database during the installation."]
["Database Name ","Entered by default","The installer created the BNA database with the name that you specify in this field, for example, bna."]
["Create New User","Unchecked by default","Check this option if you are using the Precreate database option in the installer for the BMC Network Automation installation."]
["Database User ",null,"Check this option if you are not using the Precreate database option . The installer creates a new user during the installation."]
["Password",null,"BNA database password (value is encrypted)"]
["Confirm Database Password",null,"Confirm the password you specified in the previous text box."]
["Database Administrator User Input"]
["DBA username","sa","When creating the database user and tablespace name on Linux (or database name on Windows), do not use special characters except _ and -."]
["Password","Enter required information"]
["Confirm Password","Enter required information"]
["Database Datafile","Enter the data file name with the .mdf extension","For the data file path specify the directory location upto the Data subdirectoy. For example, on Windows: C:\\Program Files\\Microsoft SQL Server\\MSSQL10_50.MSSQLSERVER\\MSSQL\\DATA\\<filename>.mdf. Note: Do not include the shared directory name in the path, for example, \\\\Z:\\BMC Software\\...ABC.mdf>"]
["Datafile Size(MB)",500]
["Datafile Max size(MB)",3000]
["Database Logfile","Enter the data file name with the .ldf extension","For the log file path specify the directory location upto the Data subdirectoy. For example, on Windows: C:\\Program Files\\Microsoft SQL Server\\MSSQL10_50.MSSQLSERVER\\MSSQL\\DATA\\<filename>.ldf. Note: Do not include the shared directory name in the path, for example, \\\\Z:\\BMC Software\\...ABC.ldf>"]
["Logfile Size(MB)",50]
["Logfile Max Size(MB)",3000]
["Certificate Information (for HTTPS certificate)"]
["  Common Name (CN)","Entered by default","Enter the host name or IPv4/IPv6 address of the server. \nNote: This field must match the host name in the URL that you use to access the BMC Network Automation web server. "]
["  Organization Unit (OU)","Entered by default","Enter the name of your organization unit. "]
["  Organization Name (O)","Entered by default","Enter the name of your organization."]
["  Locality Name (L)","Entered by default","Enter your city or other locality. "]
["  State Name (S)","Entered by default","Enter the name of your state, province, or other political subdivision. "]
["  Country (C)","Entered by default","Enter the name of your country. "]
[" Create Keystore Password","Entered by default","Enter a minimum six character password to secure the certificate keystore. Note: Record this password in a secure location. "]
["Confirm Keystore Password","Entered by default","Reenter the Keystore password."]
["Memory and System Options"]
["Initial Memory Allocation (MB)",256,"The amount of memory that the software allocates and holds upon startup. Additional memory is allocated, as needed, up to the Maximum Memory Allocation value (see next item). "]
["Maximum Memory Allocation (MB)",1024,"The maximum amount of memory that the software process can use. Use the guidelines in the Memory Guidelines table that follows to estimate the setting for initial and maximum memory based on number of devices. The actual values depend on how your system is used. If required, these values can be adjusted later. "]
["Cache Successful DNS Lookups for (seconds)",600,"The number of seconds to cache successful DNS lookups. A value of 0 caches the lookups forever. This value controls how many seconds it takes for the software to detect an IP Address change in your system when performing DNS lookups (for example, for syslog processing). Typically this value would not require a change. "]
["Additional Startup Options",null,"Additional startup options for the application. The FAQ and Knowledge Base articles might recommend additional startup options to solve issues unique to your environment. For example, if running on a headless server (no graphics card or monitor), you might have to specify -Djava.awt.headless=true for all the features of application to work properly in your environment ."]
["BBNA Post Config Installer "]
["UDDI Registry Integration Information"]
["Enable Web Services Registry Integration",null,"Optional value"]
["Web Service Endpoint URL","http://<HostName>:<Port>/uddi/services (Not selected by default)","Enter required information if you enable Web Services Registry Integration"]
["User Name","admin","Enter required information if you enable Web Services Registry Integration"]
["Password","admin","Enter required information if you enable Web Services Registry Integration"]
["Optional Service Registration Information","Not selected by default","Enter optional information if you enable Web Services Registry Integration"]
["Description","Enter required value","Enter optional information if you enable Optional Web Services Registry Information"]
["Geography","Enter required value","Enter optional information if you enable Optional Web Services Registry Information"]
["Organization","Enter required value","Enter optional information if you enable Optional Web Services Registry Information"]
["Quality of Service","Enter required value","Enter optional information if you enable Optional Web Services Registry Information"]
["AO Integration Information"]
["Enable BMC Atrium Orchestrator Integration",null,"Not selected by default"]
["Username","admin","Enter required information if you enable BMC Atrium Orchestrator Integration"]
["Password","admin123","Enter required information if you enable BMC Atrium Orchestrator Integration"]
["Grid name","GRID1","Best Practice: Change grid name to BNA_GRID."]
["Enable Continuous Compliance for Network Automation",null,"Not selected by default"]
["Create AO User Account"]
["Username","ao_adapter"]
["Password","Enter required value","Specify a value in this field if the if you enabled Create AO User Account."]
["Full Name","Atrium Orchestrator Adapter"]
["CMDB Integration Information"]
["Enable CMDB Integration",null,"Not selected by default"]
["Username","Enter required information if you enable CMDB Integration","Demo"]
["Password","Enter required information if you enable CMDB Integration"]
["CSM Integration Information"]
["Enable Virtual Data Center",null,"Not selected by default"]
["Create CSM User Account ",null,"Not selected by default"]
["Username","csm"]
["Password","Enter required information","Must be longer than 6 characters and less than 40. Applies to both Windows and Linux."]
["Full Name","csm"]
["Remote Directory Selection","C:\\Program Files\\BMC Software\\BCA-Networks","Best Practice: Change path to C:\\Program Files\\BMC Software\\BNA on Windows and /opt/bmc/bna on Linux."]

{"sheet":"Cloud Database Extensions","index":10,"n_rows":110,"n_cols":3,"rows_kept":110,"cut":false,"hidden":false,"merged":[]}
["Field in Install Planner","Default value displayed ","Comments"]
["Remote Directory Selection"]
["Remote Destination Directory ","C:\\Program Files\\BMC Software\\BMCCloudLifeCycleManagement"]
["BMC AR System Server - Cloud Database User Inputs"]
["AR System Server Administrator Name",{"$f":"$B$58","v":"Demo"}]
["AR System Server Password","Enter required value"]
["AR System Server TCP Port",0]
["AR System Server Name Alias","Entered by default","This server is the BMC AR System Server - Cloud Portal and Database primary server. "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["AR System Java Platform Information"]
["Java Plug-In Server",null,"Selected by default and cannot be disabled."]
["64-bit JRE Path (opt/java1.5/jre)","Enter required value","For example, C:\\Program Files\\Java\\jre6 (Windows) or opt/java1.5/jre (Linux)"]
["64-bit JDK Path (/opt/java1.5/jdk)","Enter required value","For example, C:\\Program Files\\Java\\jdk1.6.0_24 (Windows) or /opt/java1.5/jdk (Linux)"]
["AR System Portmapper and TCP Port Information"]
["Java Plug-in Server TCP Port Number",9999,"Must be greater than 1024"]
["Register with the Portmapper","Yes"]
["AR System Server TCP Port Number","Optional value"]
["AR System Server TCP Port Number",0]
["AR System Server Database Information"]
["Unicode Character Strings",null,"Select this option if you are installing on a Unicode database"]
["Authentication","SQL Server Authentication"]
["Host name or IP address (of database server)","Enter required value"]
["AR System Server DB port",1433]
["AR System Server DB Instance Name","Enter required value"]
["AR System Server DB Name","ARSystem"]
["AR System Server DB Log-in ID","ARAdmin"]
["AR System Server DB Password","AR#Admin#","Value is encrypted. "]
["AR System Server Administrator Information"]
["AR System Server Administrator Name","Demo"]
["AR System Server Server Password","none"]
["AR System Server Server TCP Port","Optional value"]
["AR System Server server name alias ","Enter required value","Must be registered in the DNS server."]
["Host Name or IP address (of physical system)","Enter required value"]
["DBMS Administrator Information"]
["SQL Server Administrator Login","sa"]
["SQL Server Administrator Password","Enter required value"]
["Oracle Listener Port",1521]
["Oracle Connection Identifier (Oracle alias entry in the tnsnames.ora file)","Enter required value"]
["Oracle SID or Oracle Service Name","Enter required value"]
["Directory Path for tnsnames.ora File (appears only if the installer cannot find it on ORACLE_HOME)","Enter required value"]
["AR System Server Database File Information"]
["AR System Server DB Name","ARSystem","Cannot modify this value."]
["Datafile Name","ARSys"]
["Datafile Size",500,"Each additional complex application requires an additional 2 GB of disk space."]
["Logfile Name","ARSysLog"]
["Logfile Size (MB)",100]
["AR System Password Information"]
["Local DSO User Password","Enter required value","You can change these values later in BMC Remedy Administrator Console. "]
["Application Server Password","Enter required value","You can change these values later in BMC Remedy Administrator Console. "]
["Mid-Tier Administration Password","Enter required value","You can change these values later in BMC Remedy Administrator Console. "]
["AR System Server License Information"]
["AR Server License Key","Enter required value"]
["License Expiration Date","Optional value"]
["BMC Atrium Core Installation"]
["Remote Directory Selection (BMC Atrium Core)","C:\\Program Files\\BMC Software\\AtriumCore"]
[null,"/opt/bmc/AtriumCore"]
["AR System Server Administration Priveleges"]
["AR System Server Administrator Name",{"$f":"$B$58","v":"Demo"}]
["AR System Server Password",{"$f":"$B$59","v":"none"}]
["AR System Server TCP Port",0]
["AR Server Host Name","Enter required value"]
["CMDB Plugin Server Port Information"]
["NE Plugin port",9555]
["Atrium port",9556]
["AIS Listener port",7791]
["JRE Information"]
["Use the bundled JRE (clear the check box to enter the JRE path)","Selected by default"]
["Select JRE Path","Enter required value","Make sure you use 64-bit JRE. "]
["BMC AR System Server - Cloud Database User Inputs"]
["BMC Remedy AR System User inputs"]
["AR System Server Administrator Name",{"$f":"$B$58","v":"Demo"}]
["AR System Server Password",{"$f":"$B$59","v":"none"}]
["AR System Server TCP Port",0]
["AR System Server Name Alias","Enter required value"]
["BMC Atrium Core DSO Information"]
["Destination AR Server","Enter required value"]
["Destination AR Server User",{"$f":"$B$58","v":"Demo"}]
["Destination AR Server Password",{"$f":"$B$59","v":"none"}]
["Destination AR Server Port",0]
["DSO Password","Enter required value"]
["RPC Program No","Enter required value"]

{"sheet":"Cloud Platform Manager","index":11,"n_rows":68,"n_cols":3,"rows_kept":68,"cut":false,"hidden":false,"merged":[]}
["Field in Install Planner","Default value displayed","Comments"]
["Remote Directory Selection"]
["Remote Destination Directory","C:\\Program Files\\BMC Software\\BMCCloudLifeCycleManagement"]
["BMC CLM Java Platform Information","Enter by default","Alternatively, check the Use Bundled JRE option if you have not installed JRE separately. "]
["BMC Remedy AR System - Cloud Database User Inputs"]
["AR System Server Administrator Name","Demo","Entered by default. If not, then enter the credentials for the user with Cloud AR System Server Administrator privileges."]
["AR System Server Password",null,"Entered by default. If not, then enter the password which you specified while installig the BMC Remedy AR System 8.0.00 product."]
["AR System Server TCP Port",0,"Entered by default"]
["AR System Server Name Alias","Enter required value","BMC AR System Server - Cloud Portal and Database primary host."]
["Platform Manager Configuration Directory Information"]
["Shared Directory Path","C:\\BMC Software\\BMCCloudLifeCycleManagement\\Platform_Manager\\configuration","Specify the directory in which to install the Cloud Platform Manager configuration files. Select a shared directory for HA environments."]
["OSGI Host Panel"]
["OSGI Host","Host name","Cannot modify this value."]
["OSGI Port",7070,"You can use any free port above 1024"]
["OSGI Protocol","http","You can also select https"]
["Super User password","Enter required value","Specify the Super User password for the login service. Make sure you record the password in the spreadsheet. The installer prompts for this password during Cloud Portal AR Extension installation."]
["Confirm Super User Password","Enter required value","Re-enter the password."]
["Persistence Manager Details",null,"Cloud DB Service"]
["Dataset ID","BMC.ASSET"]
["Dataset Mask",0]
["Maximum Number of Connections ",50]
["Database (AR) Server Timezone","Enter required value","For example, select America/Los_Angeles"]
["Resource Manager details"]
["BBNA Provider"]
["BBNA Server Host","bbna-hostname"]
["BBNA Server Port",443]
["BBNA Server Protocol","https","You can change the protocol to http is required."]
["BBNA User","sysadmin"]
["BBNA Password","Enter required value"]
["BBSA Provider"]
["BBSA Server Host","bbsa-hostname"]
["BBSA Web Services Port",10843]
["BBSA Server Protocol","https","You can change the protocol to http is required."]
["BBSA User","BLAdmin"]
["BBSA Password","Enter required value","Use the same password that you specified when installing BMC Server Automation - App Server & Console"]
["BBSA Role","BLAdmins"]
["BBSA registers servers by hostname",false]
["BPPM Provider"]
["BBPM Server Host","bppm-server-hostname","Specify the BPPM Central Server host name here."]
["BBPM Server Port",80]
["BBPM Server Protocol","https","You can change the protocol to http is required."]
["BBPM User","admin"]
["BBPM Password","Enter required value"]
["Callout Provider"]
["AO Server CDP URL","http://<hostname>:28080/baocdp/orca"]
["AO Server Grid Name","GRID1"]
["AO Server Username","admin"]
["AO Server Password","Enter required value","default is admin123"]
["Service Health Details"]
["SMTP host name"]
["SMTP port"]
["Sender's email address"]
["Configure BDA for BMC Cloud Lifecycle Management"]
["Do you want to configure the On-Premise Database as a Service (DBaaS) now using the installer?","No (the default)","You can still configure DBaaS later after you finish installing Compact Deployment."]
["DBaaS details",null,"Specify the details in this section if you enabled DBaaS."]
["BMC Database Automation (BDA) Manager host name"]
["User"]
["Password"]
["VCloud Enablement"]
["Do you want to enable VCloud profile?","Not enabled by default","To enable theVCloud profile, check Yes. This option helps integrating the BMC Cloud Lifecycle Management solution with the VMWare cloud director."]
["vCloud provider details",null,"Specify the details in this section if you enabled vCloud profile."]
["VCloud Server Name","Enter require value"]
["Vcloud Server Version",1.5,"The value is specified by default. "]
["VCloud default connection protocol (https/http)","https","The value is specified by default. You can specify http as the protocol is required."]
["VCloud  default protocol port",443,"Value specified by default. You can change the value if required."]
["VCloud  Administrator User Name","Enter require value"]
["VCloud  Administrator Password","Enter require value"]
["Blueprint name prefix","vCloud","Value specified by default. You can change the value if required."]

{"sheet":"Cloud Portal AR Extensions","index":12,"n_rows":34,"n_cols":3,"rows_kept":34,"cut":false,"hidden":false,"merged":[]}
["Field in Install Planner","Default value displayed","Comments"]
["Remote Directory Selection","C:\\Program Files\\BMC Software\\BMCCloudLifeCycleManagement"]
["BMC CLM Java Platform Information","Entered by default","Alternatively, check the Use Bundled JRE option if you have not installed JRE separately. "]
["BMC Remedy AR System & BMC Remedy IT Service Management Suite user inputs"]
["AR System Server Administrator Name","Demo","You can change the user name in the User form after the installation."]
["AR System Server Server Password","Enter required value"]
["AR System Server Server TCP Port",0,"Displays the BMC Remedy AR System Server TCP Port Number you entered in the BMC Remedy AR System Portmapper and TCP Port Information panel when installing  the BMC AR System Server&ITSM Suite - Primary. "]
["AR System Server Name Alias ","Entered by default                              ","The AR System host name you specify here must be registered in the DNS server.  If you are installing Cloud Portal on BMC Remedy AR System Server & ITSM Suite - Primary, use the Primary alias. Use the Secondary alias if you are installing Cloud Portal on the Secondary host."]
["Java Plugin Server TCP Port Information"]
["Java Plugin Server TCP Port Address",9899,"Must be unused, unique, and greater than 1024"]
["Super User Password"]
["Super User Password","Enter required value","Note: Specify the same value of the super user password that you entered when installing the Cloud Platform Manager login service. "]
["Confirm Super User Password","Enter required value"]
["Cloud Administrator user information"]
["Cloud Provider Company Name","CLM Provider"]
["Cloud Admin First Name","Cloud"]
["Cloud Admin Last Name","Admin"]
["Cloud Admin Login ID","clmadmin"]
["Cloud Admin Password","Enter required value"]
["Confirm Cloud Admin Password","Enter required value"]
["Atrium Orchestrator details"]
["Host","Entered by default","The default value displayed is the name of the Atrium Orchestrator host."]
["Port",28080]
["Grid Name","GRID1"]
["Administrator User","admin"]
["Administrator Password","Enter required value","admin123 by default"]
["Cloud Vista cross launch"]
["Enable Cloud Vista cross launch?","No","Select Yes to enable integration between Cloud Vista and BMC ProactiveNet Central Server."]
["Platform Manager Host Panel"]
["Platform Manager Host","platform-manager-host","Cannot modify this value."]
["Platform Manager Port",7070,"Cannot modify this value."]
["Platform Manager Protocol","http","Cannot modify this value."]
["Midtier URL details"]
["Web server URL","http://webServer:webServerPort ","URL for web server, not BMC Remedy Mid Tier (for example, http://webServer:8080). URL entered by default."]

{"sheet":"PXE Server","index":13,"n_rows":31,"n_cols":3,"rows_kept":31,"cut":false,"hidden":false,"merged":[]}
["Field in Install Planner","Default value displayed","Comments"]
["Destination Directory ","C:\\Program Files\\BMC Software\\NSH","Specify the destination directory for the BMC BladeLogic Network Shell (NSH) installation. If BMC NSH is not detected on the target host, the installer installs it as part of the PXE Server product installation.  "]
["Remote Directory Selection"]
["Remote Destination Directory ","C:\\Program Files\\BMC Software\\BladeLogic","Specify the destination directory for the PXE Server installation."]
["Database information"]
["Host name or IP address","<BMC Server Automation - Application Server & Console host name>","Specify the name of the host on which you installed the BMC Server Automation Multiple App Server (MAS)"]
["Database Port",1433]
["Database Name","BBSA","Specify the name of the BMC Server Automation database."]
["BladeLogic User","BBSAUser","Specify the name of the BMC Server Automation user that you created."]
["User Password","Enter the password that you created for the BMC Server Automation user.","Value is encrypted"]
["Confirm User Password"]
["PXE Options Information"]
["Interface to bind","eth0","The Ethernet interface that the PXE server uses to listen, for example, eth0 or eth1. Type the name of an interface. (Current active interfaces are listed above this field.) If you do not specify a valid interface, the PXE server binds to all active interfaces."]
["Multicast address","224.1.5.1","IP address of the multicast group that the PXE server listens on."]
["Listening port",4011,"Port on which the PXE server listens for connections from target machines being provisioned."]
["Prompt timeout",1,"Time (in seconds) that the boot prompt is displayed before the boot process begins."]
["PXE Server Domain",null,"Domain of the PXE server."]
["Use multicast","Selected by default","Check this option if the PXE Server should listen to multicast requests. "]
["Use broadcast",null,"Check this option if the PXE Server should listen to broadcast requests. A broadcast transmits to an entire network and thus uses network bandwidth less efficiently than a multicast."]
["TFTP Options Information"]
["IP Address","IP address that the TFTP server listens on."]
["Base Directory","C:\\Program Files\\BMC Software\\BladeLogic\\tftp","Base directory of the file system used to store operating system bootstrap programs to be downloaded."]
["MTFTP Settings","224.1.5.1","Multicast address that the TFTP server listens on."]
["Client port",1758,"Multicast port that servers being provisioned should use to communicate with the TFTP server."]
["Server port",1759,"Multicast port that the TFTP server should use to listen for communication from servers being provisioned."]
["DHCP Configuration"]
["Locally (on this server)"]
["Externally (on another server)","Selected by default"]
["Virtual Directory Creation"]
["Name","pxestore"]
["Location","C:\\Program Files\\BMC Software\\BladeLogic\\8.1\\PXE\\store"]

{"sheet":"BSA-AdvRep","index":14,"n_rows":14,"n_cols":3,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["Field in Install Planner","Default value displayed ","Comments"]
["Remote Directory Selection"]
["Remote Destination Directory","C:\\Program Files (x86)\\BMC Software\\BladeLogic\\AdvancedRepeater"]
["Workspace Directory","C:\\Program Files (x86)\\BMC Software\\BladeLogic\\AdvancedRepeater\\tuner","Specify a desination directory for BMC Server Automation - Advanced Repeater to save channels."]
["Advanced Repeater Credentials",null,"Credential settings"]
["Use default tuner credential settings",null,"Selected by default"]
["Change tuner credential settings",null,"Choose this option to change the user settings for the tuner, if required."]
["Tuner Username","Default value entered","Default value for the user name is displayed if the Use default tuner credential settings option is selected."]
["Tuner Password","Default value entered","Password is encrypted."]
["Confirm Password","Default value entered","Password is encrypted."]
["Advanced Repeater Sevice Port Numbers"]
["Transmitter RPC Port",7717]
["Transmitter Listener Port",5282]
["Proxy Listener Port",8081]

{"sheet":"BNA-Device Agent","index":15,"n_rows":19,"n_cols":3,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
["Field in Install Planner","Default value displayed ","Comments"]
["Remote Directory Selection"]
["Remote Destination Directory","C:\\Program Files\\BMC Software\\BCA-Networks-Agent"]
["RMI Port Number",null,"Port used to communicate between the BMC BladeLogic Network Automation server and device agent."]
["Port Number",1099]
["Certificate Information"]
["Common Name (CN)","Enter required value.","Enter the host name or IPv4/IPv6 address of the server. \nNote: This field must match the host name in the URL that you used to access the BMC Network Automation web server. "]
["Organization Unit (OU)","Enter required value.","Enter the name of your organization unit. "]
["Organization Name (O)","Enter required value.","Enter the name of your organization."]
["Locality Name (L)","Enter required value.","Enter your city or other locality. "]
["State Name (S)","Enter required value.","Enter the name of your state, province, or other political subdivision. "]
["Country (C)","Enter required value.","Enter the name of your country. "]
["Create Keystore Password","admin","Enter a minimum six character password to secure the certificate keystore. Note: Record this password in a secure location. "]
["Confirm Keystore Password","admin","Reenter the Keystore password."]
["Memory and System Options",null,"Amount of memory and other system options to optimize the application for your environment."]
["Initial Memory Allocation (MB)",256,"The amount of memory that the software allocates and holds upon startup. Additional memory is allocated, as needed, up to the Maximum Memory Allocation value (see next item). "]
["Maximum Memory Allocation (MB)",512,"The maximum amount of memory that the software process can use. Use the guidelines in the Memory Guidelines table that follows to estimate the setting for initial and maximum memory based on number of devices. The actual values depend on how your system is used. If required, these values can be adjusted later. "]
["Cache Successful DNS Lookups for (seconds)",600,"The number of seconds to cache successful DNS lookups. A value of 0 caches the lookups forever. This value controls how many seconds it takes for the software to detect an IP Address change in your system when performing DNS lookups (for example, for syslog processing). Typically this value would not require a change. "]
["Additional Startup Options",null,"Additional startup options for the application. The FAQ and Knowledge Base articles might recommend additional startup options to solve issues unique to your environment. For example, if running on a headless server (no graphics card or monitor), you might have to specify -Djava.awt.headless=true for all the features of application to work properly in your environment ."]